0.1a	- initial
0.2a	- support for windows 10 nvme driver (stornvme)
0.21a	- decode imft/3d flash type
0.22a	- 64L & 96L imft nand was wrong named as 32L
0.221a	- open report request
0.222t0	- sm2260/62 parameters decode
	- sm2260/62 telemetry decode
	- sm2260/62 BB & EC list binary save
	- standart nvme smart decode
	- rename standart nvme smart: smi_nvme_smart.bin to nvme_smart.bin
	- new flash type decode
0.223a	- full support connection via jms583
0.224t1	- test support for asm/rtl
0.224a	- 2263en detect
	- 2262en/b1 detect
	- EC list decode
0.225a	- CEL decode
	- skip output empty CEL
	- nvme1.3 smart attributes
0.226a	- extend EC list len
	- more telemetry params decode for 2262+
	- improve (but not completely) buffer size info decode for 2262+
	- improve smart and telemetry compatibility with stornvme driver
0.227a	- more telemetry params decode for 2262en+
	- 'n' - optional s/n output
	- preliminary support for 2267/2270
	- remove wrong page size info for YMTC nand
	- add N28A nand detect
0.228a	- decode "Critical Warning" nvme smart attribute
	- update FID decoder
	- preliminary support for 2264
0.23a	- support for asm2362/4 usb-nvme bridge connection (need new firmware for 2362)
	- bypass adata S50Lite C/K degrees smart bug
0.231a	- skip FID output for bank with (0xFF) FID
	- "press any key" request also when compatible ssd not detected
	- fixed size truncate for >2TB
0.24a	- improve dram buffer size info decode for 2262[en]/2263en/2267
	- output HMB info + status
	- output OPROM status for model w/dram buffer
	- output flash block type info for model w/dram buffer [smi_nvme_flash_id_ec.txt]
	- output pages/block, bit per cell for 2263xt
	- output sm2263xt telemetry
	- 'w' - save system block for 2263xt
	- fix die density for hynix-3d
0.241a	- improve ymtc nand fid decode
0.25a	- fix sm2265 support
	- show unknown telemetry params
	- fix intel 144L nand
0.26a	- fix EC array size for model w/dram buffer
	- update FID decoder
	- support for rtl9210[b] bridge connection (need fw.1.27+)
0.27a	- try to support sm2269xt
0.271a	- skip empty telemetry output for 2263xt
	- update FID decoder
	- try to fix detect new sm2262en/sm2264 as rom mode
	- set btype size to 32k (64k dont read with some conditions)
0.272a	- fix detect sm2264
	- update FID decoder
	- try to fix solidigm p41plus detect as buferless
0.273a	- detect sm2268xt
	- update FID decoder
0.274a	- detect sm2508
	- update FID decoder
0.2741a	- some fix for sm2508
0.275a	- detect sm8366
	- fix wrong "rom mode" for sm8366
	- detect sm2504
	- update FID decoder
